{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","Test TC160075","EGSQH10S18AA9W"]
["Uwagi","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)","(1) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)","(2) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(3) - z glikolem propylenowym 40%","(3) - Poziom ciśnienia akustycznego jest mierzony za pomocą mikrofonu z odległości 1 m od jednostki. Jest to wartość względna, zależy od odległości i warunków akustycznych."]
["","","","","","(4) - Straty ciepła według EN12897","(4) - Łącznie z instalacją + PHE + dodatkową grzałką; bez przeponowego naczynia wzbiorczego"]
["","","","","","(5) - Łącznie z instalacją + PHE + dodatkową grzałką; bez przeponowego naczynia wzbiorczego","(5) - Straty ciepła według EN12897"]
["","","","","","(6) - Poziom ciśnienia akustycznego jest mierzony za pomocą mikrofonu z odległości 1 m od jednostki. Jest to wartość względna, zależy od odległości i warunków akustycznych.","(6) - Przez pompę ciepła + dodatkowy element grzewczy"]
["","","","","","(7) - Przez pompę ciepła","(7) - Przez pompę ciepła"]
["","","","","","(8) - Przez pompę ciepła + dodatkowy element grzewczy","(8) - Przez dodatkowy element grzewczy"]
["","","","","","(9) - Przez dodatkowy element grzewczy","(9) - z glikolem propylenowym 40%"]
["Wydajność grzewcza","Min.","","","kW","","3.11, 2.47"]
["","Nom.","","","kW","","10.3, 9.2"]
["","Maks.","","","kW","","13, 11.9"]
["Pobór mocy","Nom.","","","kW","","2.38, 2.89"]
["COP","","","","","","4.33, 3.18"]
["Obudowa","Kolor","","","","","Biały"]
["Obudowa","Materiał","","","","","Arkusz metalowy z powłoką wstępną"]
["Wymiary","Jednostka","","Wysokość","mm","","1730"]
["","","","Szerokość","mm","","600"]
["","","","Głębokość","mm","","728"]
["Ciężar","Jednostka","","","kg","","210"]
["Zbiornik","Objętość wody","","","l","","180"]
["","Izolacja","","Straty ciepła","kWh/24h","","1.36"]
["","Zabezpieczenie przed korozją","","","","","Anoda"]
["Czynnik chłodniczy","Typ","","","","","R-410A"]
["Czynnik chłodniczy","GWP","","","","","2090"]
["Czynnik chłodniczy","Ilość","","","tCO2Eq","","3.76"]
["","Czynnik chłodniczy-=-Dopełnienie-=-kg","","","kg","","1.8"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","","3.68"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","A++"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 35°C","Informacje ogólne","SCOP","","","5.06"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","A+++"]
["Zasilanie energią elektryczną","Nazwa","","","","","9W"]
["","liczba faz","","","","","3~"]
["Zasilanie","Zasilanie-=-Częstotliwość","","Częstotliwość","","","50"]
["","Zasilanie-=-Napięcie","","Napięcie","","","400"]
["Prąd","Current-=-Recommended fuses","","Recommended fuses","","","25"]