{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","","FCAHG71FVEB"]
["Obudowa","Materiał","","","","Galwanizowana blacha stalowa"]
["Wymiary","Jednostka","","Wysokość","mm","288"]
["","","","Szerokość","mm","840"]
["","","","Głębokość","mm","840"]
["Ciężar","Jednostka","","","kg","25.0"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","21.2"]
["Wentylator","Przepływ powietrza","Chłodzenie","Medium","m³/min","16.7"]
["Wentylator","Przepływ powietrza","Chłodzenie","Niski","m³/min","12.2"]
["","","Grzanie","Wysoki","m³/min","21.2"]
["Wentylator","Przepływ powietrza","Grzanie","Medium","m³/min","16.7"]
["Wentylator","Przepływ powietrza","Grzanie","Niski","m³/min","12.2"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","53"]
["","Ogrzewanie","","","dBA","53"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","36"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Medium","dBA","33"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Niski","dBA","29"]
["","Grzanie","","Wysoki","dBA","36"]
["","Ogrzewanie","","Czynnik","dBA","33"]
["","Grzanie","","Niski","dBA","29"]
["Czynnik chłodniczy","GWP","","","","675"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52"]
["Połączenia instalacji","Gaz","","Śr. zewn.","mm","15.9"]
["Połączenia instalacji rurowej","Spust","","","","VP25 (I.D. 25/O.D. 32)"]
["Panel dekoracyjny","Model","","","","BYCQ140D7GFW1 - Panel z funkcja automatycznego czyszczenia, drobniejszą siatką filtracyjną"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","130"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","950"]
["","Ciężar","","","kg","10"]
["Panel dekoracyjny 2","Model","","","","BYCQ140D7GW1 - panel z funkcją automatycznego czyszczenia"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","130"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","950"]
["","Ciężar","","","kg","10.3"]
["Panel dekoracyjny 3","Model","","","","BYCQ140D7W1W - cały biały, Patrz Uwaga 1"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","50"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","950"]
["","Ciężar","","","kg","5.4"]
["Panel dekoracyjny 4","Model","","","","BYCQ140D7W1 - biały z szarymi żaluzjami"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","50"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","950"]
["","Ciężar","","","kg","5.4"]
["Standardowe akcesoria","Installation manual","","","","Installation manual"]
["","Installation and operation manual","","","","Installation and operation manual"]
["Zasilanie energią elektryczną","Nazwa","","","","VE"]
["","liczba faz","","","","1~"]
["Zasilanie","Zasilanie-=-Częstotliwość","","Częstotliwość","","50/60"]
["","Zasilanie-=-Napięcie","","Napięcie","","220-240"]