{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":99,"n_cols":7,"rows_kept":99,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BS","FTXJ50MV1BS"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","47"]
["","","","Czynnik","dBA","","41"]
["","","","Cicha praca","dBA","","25"]
["","","","Niski","dBA","","35"]
["","Chłodzenie","","Medium","dBA","","40"]
["","","","Cicha praca","dBA","","25"]
["","","","Niski","dBA","","35"]
["","","","Wysoki","dBA","","46"]
["Standardowe akcesoria","Instrukcja obsługi","","","","","1"]
["","Instrukcja instalacji","","","","","1"]
["","Pilot bezprzewodowy","","","","","1"]
["","Baterie suche typu AAA","","","","","2"]
["","Uchwyt do pilota","","","","","1"]
["","Śruby mocujące płytę montażową","","","","","5"]
["","Płyta montażowa","","","","","1"]
["","Tytanowo-apatytowy filtr eliminujący zapachy","","","","","2"]
["","Śruba mocująca dla uchwytu zdalnego sterownika","","","","","2"]
["","Śruby mocujące jednostkę wewnętrzną","","","","","2"]
["","Pokrywa na śruby","","","","","2"]
["","Zestaw adaptera WLAN","","","","","1"]
["Control systems","Infrared remote control","","","","","ARC466A9"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","","6.35"]
["","Gaz","","Śr. zewn.","mm","","12.70"]
["","Spust","","","","","18"]
["Power input","Chłodzenie","","Nom.","kW","","0.033"]
["","Grzanie","","Nom.","kW","","0.043"]
["Sound power level","Chłodzenie","","","dBA","","60"]
["","Ogrzewanie","","","dBA","","60"]
["Wymiary","Jednostka","","Szerokość","mm","","998"]
["","","","Głębokość","mm","","212"]
["","","","Wysokość","mm","","303"]
["Obudowa","Kolor","","","","","Srebrny"]
["Ciężar","Jednostka","","","kg","","12"]
["Wentylator","Przepływ powietrza","Grzanie","Wysoki","m³/min","","12.6"]
["","","","Medium","m³/min","","10.5"]
["","","","Niski","m³/min","","8.1"]
["","","","Cicha praca","m³/min","","5.0"]
["","","Chłodzenie","Niski","m³/min","","6.8"]
["","","","Medium","m³/min","","8.9"]
["","","","Wysoki","m³/min","","10.9"]
["","","","Cicha praca","m³/min","","3.6"]
["Power supply","liczba faz","","","","","1~"]
["","Nazwa","","","","","V1"]
["","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.023"]
["","Grzanie","","Nom.","kW","0.031"]
["Obudowa","Kolor","","","","Srebrny"]
["Wymiary","Jednostka","","Wysokość","mm","303"]
["","","","Szerokość","mm","998"]
["","","","Głębokość","mm","212"]
["Ciężar","Jednostka","","","kg","12"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","8.9"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","6.6"]
["","","","Niski","m³/min","4.4"]
["","","","Cicha praca","m³/min","2.6"]
["","","Grzanie","Wysoki","m³/min","10.2"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","8.4"]
["","","Grzanie","Niski","m³/min","6.3"]
["","","","Cicha praca","m³/min","3.8"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","54"]
["","Ogrzewanie","","","dBA","56"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","38"]
["","","","Czynnik","dBA","32"]
["","","","Niski","dBA","25"]
["","","","Cicha praca","dBA","19"]
["","Grzanie","","Wysoki","dBA","40"]
["","Ogrzewanie","","Czynnik","dBA","34"]
["","Grzanie","","Niski","dBA","28"]
["","","","Cicha praca","dBA","19"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35"]
["","Gaz","","Śr. zewn.","mm","9.50"]
["","Spust","","","","18"]
["Syst. kontroli","Pilot na podczerwień","","","","ARC466A9"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","Fixing screw for remote controller holder","","","","2"]
["","WLAN adapter kit","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Fixing screws for mounting plate","","","","5"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1"]
["","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]