{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BW","FTXJ25MV1BW","FTXJ35MV1BW","FTXJ50MV1BW"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","40","41","45","47"]
["","","","Czynnik","dBA","34","34","37","41"]
["","","","Cicha praca","dBA","19","19","20","25"]
["","","","Niski","dBA","28","28","29","35"]
["","Chłodzenie","","Medium","dBA","32","32","34","40"]
["","","","Cicha praca","dBA","19","19","20","25"]
["","","","Niski","dBA","25","25","26","35"]
["","","","Wysoki","dBA","38","38","45","46"]
["Standardowe akcesoria","Instrukcja obsługi","","","","1","1","1","1"]
["","Instrukcja instalacji","","","","1","1","1","1"]
["","Pilot bezprzewodowy","","","","1","1","1","1"]
["","Baterie suche typu AAA","","","","2","2","2","2"]
["","Uchwyt do pilota","","","","1","1","1","1"]
["","Śruby mocujące płytę montażową","","","","5","5","5","5"]
["","Płyta montażowa","","","","1","1","1","1"]
["","Tytanowo-apatytowy filtr eliminujący zapachy","","","","2","2","2","2"]
["","Śruba mocująca dla uchwytu zdalnego sterownika","","","","2","2","2","2"]
["","Śruby mocujące jednostkę wewnętrzną","","","","2","2","2","2"]
["","Pokrywa na śruby","","","","2","2","2","2"]
["","Zestaw adaptera WLAN","","","","1","1","1","1"]
["Control systems","Infrared remote control","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.50","9.50","9.50","12.70"]
["","Spust","","","","18","18","18","18"]
["Power input","Chłodzenie","","Nom.","kW","0.023","0.023","0.033","0.033"]
["","Grzanie","","Nom.","kW","0.031","0.033","0.042","0.043"]
["Sound power level","Chłodzenie","","","dBA","54","54","59","60"]
["","Ogrzewanie","","","dBA","56","56","59","60"]
["Wymiary","Jednostka","","Szerokość","mm","998","998","998","998"]
["","","","Głębokość","mm","212","212","212","212"]
["","","","Wysokość","mm","303","303","303","303"]
["Obudowa","Kolor","","","","Biały","Biały","Biały","Biały"]
["Ciężar","Jednostka","","","kg","12","12","12","12"]
["Wentylator","Przepływ powietrza","Grzanie","Wysoki","m³/min","10.2","11.0","12.4","12.6"]
["","","","Medium","m³/min","8.4","8.6","9.6","10.5"]
["","","","Niski","m³/min","6.3","6.3","6.9","8.1"]
["","","","Cicha praca","m³/min","3.8","3.8","4.1","5.0"]
["","","Chłodzenie","Niski","m³/min","4.4","4.4","4.8","6.8"]
["","","","Medium","m³/min","6.6","6.6","7.8","8.9"]
["","","","Wysoki","m³/min","8.9","8.9","10.9","10.9"]
["","","","Cicha praca","m³/min","2.6","2.6","2.9","3.6"]
["Power supply","liczba faz","","","","1~","1~","1~","1~"]
["","Nazwa","","","","V1","V1","V1","V1"]
["","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]