{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M"]
[]
[]
[]
[]
["","","","","","FTXM42M2V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.035"]
["","Grzanie","","Nom.","kW","0.035"]
["Obudowa","Kolor","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","294"]
["","","","Szerokość","mm","811"]
["","","","Głębokość","mm","272"]
["Ciężar","Jednostka","","","kg","10"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","12.6"]
["Wentylator","Przepływ powietrza","Chłodzenie","Medium","m³/min","9.5"]
["Wentylator","Przepływ powietrza","Chłodzenie","Niski","m³/min","7.1"]
["","","","Cicha praca","m³/min","4.6"]
["","","Grzanie","Wysoki","m³/min","13"]
["Wentylator","Przepływ powietrza","Grzanie","Medium","m³/min","10.4"]
["Wentylator","Przepływ powietrza","Grzanie","Niski","m³/min","7.1"]
["","","","Cicha praca","m³/min","5.3"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","60"]
["","Ogrzewanie","","","dBA","60"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","45"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Medium","dBA","39"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Niski","dBA","30"]
["","","","Cicha praca","dBA","21"]
["","Grzanie","","Wysoki","dBA","45"]
["","Ogrzewanie","","Czynnik","dBA","39"]
["","Grzanie","","Niski","dBA","29"]
["","","","Cicha praca","dBA","21"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35"]
["Połączenia instalacji","Gaz","","Śr. zewn.","mm","12.7"]
["Połączenia instalacji rurowej","Spust","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A33"]
["","Wired remote control","","","","BRC944B2, BRC073A1"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1"]
["","liczba faz","","","","1~"]
["Zasilanie","Zasilanie-=-Częstotliwość","","Częstotliwość","","50"]
["","Zasilanie-=-Napięcie","","Napięcie","","220-240"]