{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-LV1"]
[]
[]
[]
[]
["","","","","","RZAG71L7V1B"]
["Wymiary","Jednostka","","Wysokość","mm","990"]
["","","","Szerokość","mm","940"]
["","","","Głębokość","mm","320"]
["Ciężar","Jednostka","","","kg","67"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-15"]
["","","","Maks.","°CDB","50"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-20"]
["","","","Maks.","°CWB","15.5"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","64"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","48"]
["","Grzanie","","Nom.","dBA","50"]
["","Tryb nocny","","Poziom 1","dBA","43"]
["Czynnik chłodniczy","Typ","","","","R-32"]
["","Czynnik chłodniczy-=-Dopełnienie-=-kg","","","kg","2.6"]
["Czynnik chłodniczy","GWP","","","","675"]
["Czynnik chłodniczy","Ilość","","","tCO2Eq","1.8"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52"]
["Połączenia instalacji","Gaz","","Śr. zewn.","mm","15.9"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","55"]
["","Dugo instalacji rurowej","System","Równoważnik","m","75"]
["Podłączenie instalacji rurowej","Długość instalacji rurowej","System","Podłączenie instalacji rurowej-=-Długość instalacji rurowej-=-System-=-Bez obciążenia-=-m","m","30"]
["Połączenia instalacji","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","Patrz instrukcja instalacji"]
["","Różnica poziomów","IU - OU","Maks.","m","30.0"]
["","","IU - IU","Maks.","m","0.5"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Zasilanie-=-Częstotliwość","","Częstotliwość","","50/60"]
["","Zasilanie-=-Napięcie","","Napięcie","","220-240"]